**ARDON®CREATRON®**

TROUSERS



**TECHNICAL DATA SHEET**

**ARDON®CREATRON®**

TROUSERS

**ARTICLE** H6650 (black-neon)

**MATERIAL** 98 % cotton, 2 % elastane, Amalytton®, canvas

**GRAMMAGE** 250 g/m2

**SIZE** 46-64

**DESCRIPTION**

Stretch cotton waist working trousers made from the special Amalytton® material that features increased strength and a smooth, soft surface. The reduced grammage means the trousers are very pleasant to wear, which you will appreciate not just in summer when it is hot. The exposed areas are made of the Tabiflex® extra durable and four- -way stretch material. The trousers have a highly functional ergonomic 3D cut that accentuates the silhouette. The knee area is reinforced with durable Oxford material treated with a water repellent additive; the knee pocket can be used for inserting knee pads. They feature an elastic waistband along with a concealed rear double belt loop for a comfortable belt fit, a D-ring snap-hook, 2 hidden pockets, 1 front zip pocket, 1 front tool pocket with a wide loop, a multifunctional pocket for a folding tape measure, screwdriver and snap-off knife with wide loops on the right leg, and a large double pocket covered with a snap flap on the left leg. The back part consists of a yoke and 2 pockets, the right back pocket is covered with a snap flap. The lower leg hem is reinforced with the abrasion-resistant Oxford material. Dynamic high-visibility 3D printing and accessories provide increased user visibility. The leg length can be easily extended by 5 cm.

This personal protective equipment is in conformity with the requirements of the following harmonised standard:

**TECHNICAL DATA SHEET**

**ČSN EN ISO 13688:2013** – Protective clothing - General requirements

PPE of simple design against the minimum risks that may be quickly

and safety recognised by the user.

The self-certification was carried out on the basis of the technical documentation of the product and practical tests of ergonomics propreties of the product by Ardon Safety s.r.o. on 20 January 2021.

The CREATRON Collection meets health requirements and is **OEKO-TEX®Standard 100 certified, PG020 certificate 128167 OETI.**

**NUMBER OF PIECES IN CARTON** 20 pcs

**CARTON WEIGHT** 20 kg

**CARTON SIZE** 0,085 m3

**UNIT PACKAGING** 1 pc

The service life depends on the rate of use and the rate of wear in the given

conditions. Inapropriate storage conditions, improper maintenance and care

reduce the service life. The warranty period is 24 months. Under no circumstances

should the warranty period be confused with the service lefe of the product. With

Intensive use, the service life may be shorter than the warranty provided.

The product does not contain any substances in concentrations that are known or

suspected to have an adverse effect on the user´s hygiene of health. However, skin

irritation is not impossible for sensitive people, in which case do not continue to

use the garment. Avoid the fire and sources of intense heat. No accessories or

replacement pants are intended for these garments. If the garment is not in use, it

Is recommended to store it in a dry and well-ventilated area away from direct

Sunlight. Transport best in original packaging, protect from moisture and extreme

temperatures. Dispose ecologically after use.

**TECHNICAL DATA SHEET**



**TECHNICAL DATA SHEET**